- Top
- Notes
- Updating the camera firmware

# Updating the camera firmware

Confirm the firmware version of the camera in the [SYSTEM SETTINGS] menu → [INFORMATION] → [VERSION], and access the most current information regarding firmware in the website described in NOTE, and download the firmware if required.

NOTE

- Update is completed by loading the downloaded file to the camera via the SD card. Insert the SD card that stores the update file into the card slot 1, and select the [SYSTEM SETTINGS] menu → [INFORMATION] → [UPDATE]. For update method, refer to the support desk at the following website:

  https://pro-av.panasonic.net/

- Always perform update of the firmware with the LCD monitor unit mounted.

- When updating the firmware, use the AC adaptor or sufficiently charged battery.

- Do not turn off the power while updating the firmware. Rewriting of the firmware may fail and the camera may not be activated.

Top of the page