- Top
- Shooting
- Image quality adjustment

# Image quality adjustment

The image quality of the video to be recorded can be adjusted in the camera when the [SYSTEM SETTINGS] menu → [COLOR SETTINGS] → [MAIN] → [SCENE1] to [SCENE5]is set.

- Adjust the image quality in the [CAMERA SETTINGS] menu.

- The [SCENE FILE SETTINGS] menu cannot be set when [MAIN] is set to [V-Log].

- It is necessary to use a measuring device such as vector scope to change the setting.

- Meaning of the symbols used in the table are as follows.

  ✓: Can be set.

  —: Cannot be set.

Item | The [SCENE FILE SETTINGS] menu → [GAMMA] → [GAMMA SELECT]
--- | ---
[V-255570L1] [V-504580L1] | [VIDEO] | [HLG]
The [SCENE FILE SETTINGS] menu
[NAME EDIT] | ✓ | ✓ | ✓
[BLACK] | ✓ | ✓ | ✓
[GAMMA] | [MASTER GAMMA] | — | ✓ | —
[BLACK GAMMA] | — | ✓ | ✓
[B.GAMMA RANGE] | — | ✓ | ✓
[KNEE] | — | ✓ | —
[HLG KNEE] | — | — | ✓
[WHITE CLIP] | — | ✓ | —
[DETAIL] | ✓ | ✓ | ✓
[SKIN DETAIL] | ✓ | ✓ | ✓
[CHROMA] | ✓ | ✓ | ✓
[MATRIX] | ✓ | ✓ | ✓
[COLOR CORRECTION] | ✓ | ✓ | ✓

[EI]
[WHITE]
[BLACK]
[GAMMA]
[KNEE]
[HLG KNEE]
[WHITE CLIP]
[DETAIL]
[SKIN DETAIL]
[CHROMA]
[MATRIX]
[COLOR CORRECTION]
Top of the page