- Top
- Operation
- Target items for scene file/setup file/initialization
- [OUTPUT SETTINGS] menu

# [OUTPUT SETTINGS] menu

Item | SCENE | SETUP | INITIALIZE
--- | --- | --- | ---
[SDI OUT] | [OUTPUT SW] | — | ✓ | ✓
| [SIGNAL SEL] | — | ✓ | ✓
| [OUT FORMAT] | — | ✓ | ✓
| [3G-SDI OUT] | — | ✓ | ✓
| [SDI REC REMOTE] | — | ✓ | ✓
| [INDICATOR DISP] | — | ✓ | ✓
| [MARKER DISP] | — | ✓ | ✓
| [MENU DISP] | — | ✓ | ✓
| [SDI OUT HDR] | — | ✓ | ✓
[HDMI OUT] | [SIGNAL SEL] | — | ✓ | ✓
| [OUT FORMAT] | — | ✓ | ✓
| [HDMI TC OUT] | — | ✓ | ✓
| [HDMI REC REMOTE] | — | ✓ | ✓
| [INDICATOR DISP] | — | ✓ | ✓
| [MARKER DISP] | — | ✓ | ✓
| [MENU DISP] | — | ✓ | ✓
| [HDMI OUT HDR] | — | ✓ | ✓
[LCD HDR] | — | ✓ | ✓
[SDI/HDMI INDICATOR] | [CLIP NAME] | — | ✓ | ✓
| [PIXEL/FREQ] | — | ✓ | ✓
| [MAIN COLOR] | — | ✓ | ✓
| [REC FORMAT] | — | ✓ | ✓
| [SLOT1/2 STATUS] | — | ✓ | ✓
| [2 SLOTS FUNC.] | — | ✓ | ✓
| [TC] | — | ✓ | ✓
| [BATTERY REMAIN] | — | ✓ | ✓
| [REC MODE] | — | ✓ | ✓
| [REC REMOTE] | — | ✓ | ✓
| [AUDIO LEVEL METER] | — | ✓ | ✓
| [FPS] | — | ✓ | ✓
| [SHUTTER] | — | ✓ | ✓
| [EI] | — | ✓ | ✓
| [WHITE] | — | ✓ | ✓
| [IRIS/ZOOM] | — | ✓ | ✓
| [FOCUS] | — | ✓ | ✓
| [ND FILTER] | — | ✓ | ✓
| [E.I.S./D.ZOOM] | — | ✓ | ✓
| [WLAN] | — | ✓ | ✓
| [IR SHOOTING] | — | ✓ | ✓
| [SPOT METER] | — | ✓ | ✓
| [PLAYBACK STATUS] | — | ✓ | ✓
[SDI/HDMI MARKER] | [CENTER MARKER] | — | ✓ | ✓
| [SAFETY MARKER] | — | ✓ | ✓
| [SAFETY AREA] | — | ✓ | ✓
| [FRAME MARKER] | — | ✓ | ✓
| [FRAME COLOR] | — | ✓ | ✓
| [PLAYBACK MARKER] | — | ✓ | ✓
[LCD INDICATOR] | [CLIP NAME] | — | ✓ | ✓
| [PIXEL/FREQ] | — | ✓ | ✓
| [MAIN COLOR] | — | ✓ | ✓
| [REC FORMAT] | — | ✓ | ✓
| [SLOT1/2 STATUS] | — | ✓ | ✓
| [2 SLOTS FUNC.] | — | ✓ | ✓
| [TC] | — | ✓ | ✓
| [BATTERY REMAIN] | — | ✓ | ✓
| [REC MODE] | — | ✓ | ✓
| [REC REMOTE] | — | ✓ | ✓
| [AUDIO LEVEL METER] | — | ✓ | ✓
| [FPS] | — | ✓ | ✓
| [SHUTTER] | — | ✓ | ✓
| [EI] | — | ✓ | ✓
| [WHITE] | — | ✓ | ✓
| [IRIS/ZOOM] | — | ✓ | ✓
| [FOCUS] | — | ✓ | ✓
| [ND FILTER] | — | ✓ | ✓
| [E.I.S./D.ZOOM] | — | ✓ | ✓
| [WLAN] | — | ✓ | ✓
| [IR SHOOTING] | — | ✓ | ✓
| [SPOT METER] | — | ✓ | ✓
| [PLAYBACK STATUS] | — | ✓ | ✓
[LCD MARKER] | [CENTER MARKER] | — | ✓ | ✓
| [SAFETY MARKER] | — | ✓ | ✓
| [SAFETY AREA] | — | ✓ | ✓
| [FRAME MARKER] | — | ✓ | ✓
| [FRAME COLOR] | — | ✓ | ✓
| [PLAYBACK MARKER] | — | ✓ | ✓
[LCD FOCUS ASSIST] | [EXPAND MODE] | — | ✓ | ✓
| [EXPAND VALUE] | — | ✓ | ✓
| [PEAK./SQUARES MODE] | — | ✓ | ✓
| [PEAKING LEVEL] | — | ✓ | ✓
| [PEAKING COLOR] | — | ✓ | ✓
| [BLACK & WHITE] | — | ✓ | ✓
| [OPEN IRIS MODE] | — | ✓ | ✓
[LCD EI ASSIST] | [ZEBRA] | — | ✓ | ✓
| [ZEBRA1 DETECT] | — | ✓ | ✓
| [ZEBRA2 DETECT] | — | ✓ | ✓
| [ZEBRA2] | — | ✓ | ✓
| [WFM MODE] | — | ✓ | ✓
| [WFM TRANSPARENCE] | — | ✓ | ✓
| [SPOT METER UNIT] | — | ✓ | ✓
| [SPOT METER SIZE] | — | ✓ | ✓
[LCD LEVEL GAUGE] | [LEVEL GAUGE] | — | ✓ | ✓
[LEVEL GAUGE RESET] | — | — | —
[COLOR BARS] | [COLOR BARS TYPE] | — | ✓ | ✓
[TEST TONE] | — | ✓ | ✓

Top of the page