- Top
- Preparation
- Preparing the SD card
- SD cards supported on the camera

# SD cards supported on the camera

Following SD cards can be used with the camera. (As of April 2022)

Type of the SD card | Recording capacity
--- | ---
SDHC memory card | 4 GB - 32 GB
SDXC memory card | 48 GB - 128 GB

- Operation is not guaranteed for any SD cards other than above.

- It is recommended to use the Panasonic SD card.

- Following SD cards cannot be used since they are not compliant with the SD standards.

  - SD card with 4 GB or larger without SDHC logo display

  - SD card with 48 GB or larger without SDXC logo display

## Speed Class during shooting

The SD card to be used differs depending on the recording mode and the recording format.

Use the SD card compatible to the Speed Class, UHS Speed Class, or Video Speed Class.

The recording may stop suddenly when the SD card not compatible to required Speed Class is used.

- Speed Class, UHS Speed Class, and Video Speed Class are the speed specification regarding continuous writing. It can be checked at the display on the SD card label, etc.

#### When the recording mode is MOV

SDXC memory card can be used.

Recording bit rate or recording function | Speed Class | Example of card display
--- | --- | ---
400 Mbps | Video Speed Class V60 or higher |
2K/FHD VFR ALL-I (Variable frame rate recording)
200 Mbps | Video Speed Class V30 or higher, UHS Speed Class 3 or higher |
150 Mbps
100 Mbps
2K/FHD VFR LongGOP (Variable frame rate recording)
50 Mbps | Video Speed Class V10 or higher, UHS Speed Class 1 or higher, Speed Class 10 or higher |

#### When the recording mode is AVCHD

SDHC memory card and SDXC memory card can be used.

Recording bit rate or recording function | Speed Class | Example of card display
--- | --- | ---
All | Speed Class 4 or higher |

Top of the page