- Top
- Notes
- Frequently asked questions
- Power supply

# Power supply

#### What is the power supply voltage supported by the supplied AC adaptor?

- AC 100 V-240 V

#### Can the supplied AC adaptor used while the battery is mounted?

- It can be used. Supplying of the power is automatically switched to the AC adaptor side when the power is set to < > (ON) and the AC adaptor is connected while the battery is mounted.

  The power status display in the LCD monitor will change from the mark to the .

#### The camera cannot be operated even when the power is set to < > (ON).

- Remove the power supply (the battery or the AC adaptor), and connect it again after approximately one minute.

- The operation of the corresponding button or the switch is disabled when the <LOCK> switch on the camera is set to < >. Unlock if necessary.

Top of the page