- Top
- Shooting
- Image quality adjustment
- [GAMMA]

# [GAMMA]

## [GAMMA SELECT]

Set to optimize the tone of video.

The items that can be selected differ depending on the [SYSTEM SETTINGS] menu → [COLOR SETTINGS] → [MAIN] setting.

Output (%)

Input/Stop

[V-Log]

[V-255570L1] ([SCENE1]: EVA-LOOK)

[V-504580L1] ([SCENE2]: EVA-LOOK)

Output (%)

[VIDEO] ([SCENE3]/[SCENE4]: BC-LOOK)

[KNEE SW] = [ON]

[KNEE POINT] = [85%]

[KNEE SLOPE] = [100]

Input/dynamic range (%)

Output (%)

Input/dynamic range (%)

[HLG] ([SCENE5]: HDR)

- [V-Log]

  This is a gamma curve that can achieve gradation and wide latitude (exposure range). A grading process after recording is required.

- [V-255570L1]

  This is the EVA-LOOK gamma curve with 14Stop latitude equivalent to [V-Log].

  The rise is equivalent to approximately 2.5 times, and the gamma factor is 0.55, which means up to 70%.

  This is a setting focused on contrast.

  It is recommended to shoot at 40% to 55% for face tone.

- [V-504580L1]

  This is the EVA-LOOK gamma curve with 14Stop latitude equivalent to [V-Log].

  The rise is equivalent to approximately 5.0 times, and the gamma factor is 0.45, which means up to 80%.

  This is a setting focused on soft texture.

  It is recommended to shoot at 40% to 60% for face tone.

- [VIDEO]

  This is the BroadCast-LOOK gamma curve with 600% dynamic range equivalent to the generally used video camera.

- [HLG]

  this is the hybrid log gamma curve with wide dynamic range of 1200%.

  The color range equivalent to BT.2020 is automatically set.

  #### When [MAIN] is set to [V-Log]

  [GAMMA] will be set to [V-Log].

  #### When [MAIN] is set to [SCENE1]/[SCENE2]/[SCENE3]/[SCENE4]/[SCENE5]

  Select the [SCENE FILE SETTINGS] menu → [GAMMA] → [GAMMA SELECT].

  Select one from [V-255570L1]/[V-504580L1]/[VIDEO]/[HLG].

## [MASTER GAMMA]

This can be set when the [SCENE FILE SETTINGS] menu → [GAMMA] → [GAMMA SELECT] → [VIDEO] is selected.

Fine adjusts the entire gamma curve.

## [BLACK GAMMA]

This can be set when the [SCENE FILE SETTINGS] menu → [GAMMA] → [GAMMA SELECT] → [VIDEO]/[HLG] is selected.

#### [BLACK GAMMA]

Sets the gamma curve compression and expansion of dark area.

Dark area is compressed in the negative side, and expanded in positive side.

#### [B.GAMMA RANGE]

Sets the maximum of compression and expansion in [BLACK GAMMA].

Top of the page