- Top
- Shooting
- Audio input
- Switching the audio input

# Switching the audio input

#### Audio recording format

The audio recording format such as compression format varies depending on the recording mode.

Recording mode | Recording format | Sampling rate/bit
--- | --- | ---
MOV | Linear PCM (LPCM) | 48 kHz/24 bit
AVCHD | Dolby AudioTM | 48 kHz/16 bit

#### Selecting audio input signals

The recorded input signal varies depending on the [AUDIO SETTINGS] menu → [AUDIO CH SETTINGS] → [CH1 IN SELECT]/[CH2 IN SELECT] setting.

Item | Input signal to be recorded
--- | ---
[CH1 IN SELECT] | [CH2 IN SELECT] | Audio channel 1 | Audio channel 2
[INT(L)] | [INT(R)] | Built-in microphone <L> | Built-in microphone <R>
[INPUT1] | Built-in microphone <L> | <AUDIO INPUT 1> terminal
[INPUT2] | Built-in microphone <L> | <AUDIO INPUT 2> terminal
[INPUT1] | [INT(R)] | <AUDIO INPUT 1> terminal | Built-in microphone <R>
[INPUT1] | <AUDIO INPUT 1> terminal | <AUDIO INPUT 1> terminal
[INPUT2] | <AUDIO INPUT 1> terminal | <AUDIO INPUT 2> terminal

Top of the page