- Top
- Operation
- Basic operation of the menu
- Configuration of the menu

# Configuration of the menu

## Menu types and how to open them

Menu type | Use | How to open
--- | --- | ---
Menu | The menu is structured in categorized levels according to intended use and setting frequency. | Displayed by pressing the <MENU> button. Displayed by touching the LCD monitor for one second or more and releasing it while the VIEW screen is displayed.
[OPTION] menu | A special menu is prepared considering additional functions in the future. | Displayed by pressing the <MENU> button while holding down the <EXIT> button.

## Configuration of the menu

[THUMBNAIL] menu | Performs confirmation or deleting of the recording clip. This menu can be set when the thumbnail screen is displayed.
[SYSTEM SETTINGS] menu | Sets the system in general.
[CAMERA SETTINGS] menu | Sets the basic function of the camera. This menu cannot be set when the thumbnail screen is displayed.
[SCENE FILE SETTINGS] menu | Sets the setting regarding scene file. This menu sets the detailed image quality adjustment of the camera video. Also, selection of the scene file, writing the scene file data to the camera memory, and reading from the camera memory can be performed. This menu cannot be set when the thumbnail screen is displayed.
[REC SETTINGS] menu | Sets the various items in the recording function.
[AUDIO SETTINGS] menu | Sets the input/output function of audio.
[OUTPUT SETTINGS] menu | Sets the display content or output format of the video.
[FILE] menu | Saves and reads the setting data.
[NETWORK SETTINGS] menu | Sets the setting regarding the network function.

Top of the page