- Top
- Playback
- Thumbnail operation
- Copying clips

# Copying clips

Clip can be copied between the SD cards.

Only the clip recorded in AVCHD can be copied.

Fig. 1

Fig. 2

Fig. 3

Fig. 4

Fig. 5

Press the <THUMBNAIL> button.

The thumbnail screen is displayed.

Press the <MENU> button while the thumbnail screen is displayed.

The menu is displayed.

Select the [THUMBNAIL] menu → [CLIP] → [COPY].

Select [SELECT]. (Fig. 1)

- Selecting [ALL] will copy all the clips between the SD cards.

Select the card slot for the copy destination. (Fig. 2)

The clips in the SD card of the copy source is displayed in the thumbnail screen. (Fig. 3)

- [SLOT1→SLOT2]: Clip can be copied from the SD card in the card slot 1 to the SD card in the card slot 2.

- [SLOT2→SLOT1]: Clip can be copied from the SD card in the card slot 2 to the SD card in the card slot 1.

Select the clip to copy in the thumbnail screen.

is displayed on the selected clip.

Select . (Fig. 4)

- This can also be selected by pressing and holding the multidial.

When the confirmation message is displayed, select [SET].

Progress bar is displayed, and the copy of the clip starts.

- To cancel the copy midway, select [CANCEL].

When the completion message is displayed, select . (Fig. 5)

NOTE

- The clip with MOV as the recording codec cannot be copied.

- The copy is not possible when the volume of the selected clip is larger than the available card capacity of the destination.

- It cannot copy when the copy destination card is write protected.

- The copy is not possible when the maximum number of the clips will exceed.

- The copy is not possible when the maximum number of the playlist will exceed.

Top of the page