- Top
- Specification
- Specifications
- Memory card recorder

# Memory card recorder

Recording media | Card slot × 2 SDHC memory card (4 GB - 32 GB) SDXC memory card (exceeding 32 GB - 128 GB) : UHS-I/UHS-II, UHS Speed Class 3 compatible, video Speed Class V90 compatible
Number of recording pixels | 4096×2160 (4K), 3840×2160 (UHD), 2048×1080 (2K), 1920×1080 (FHD), 1280×720 (HD)
Recording codec | MOV, AVCHD
System frequency | 59.94p, 59.94i, 50p, 50i, 29.97p, 24p, 25p, 23.98p
Recording frame rate (max) | 4K/UHD 59.94fps or 50fps 2K/HD 120fps/100fps 240fps/200fps (crop mode)
Recording format | MOV: 4:2:0 (10 bits) HEVC LongGOP 200M/HEVC LongGOP 150M MOV: 4:2:0 (8 bits) 420LongGOP 150M/420LongGOP 100M/420LongGOP 50M MOV: 4:2:2 (10 bits) 422LongGOP 150M/422LongGOP 100M/422LongGOP 50M 422ALL-I 400M/422ALL-I 200M/422ALL-I 100M AVCHD: PS/PH/HA/PM
Recording video signal | 4096×2160/59.94p, 50p, 29.97p, 25p, 24p, 23.98p 3840×2160/59.94p, 50p, 29.97p, 25p, 23.98p 2048×1080/59.94p, 50p, 29.97p, 25p, 24p, 23.98p 1920×1080/59.94p, 50p, 29.97p, 25p, 23.98p, 59.94i, 50i 1280×720/59.94p, 50p
Recording and playback time | When using a 64 GB SDXC memory card 4096×2160/422ALL-I 400M/29.97p, 25p, 23.98p, 24p Approx. 20 minutes 2048×1080/422ALL-I 200M/59.94p, 50p Approx. 40 minutes 4096×2160/420LongGOP 150M/59.94p, 50p Approx. 55 minutes 2048×1080/420LongGOP 100M/59.94p, 50p Approx. 1 hour 20 minutes 1920×1080/420LongGOP 50M/29.97p, 25p, 23.98p Approx. 2 hours 40 minutes
Two-slot function | Simultaneous recording, relay recording
Special recording | Pre-recording, interval recording

Top of the page