- Top
- Preparation
- Preparing the SD card
- Inserting/removing of the SD card

# Inserting/removing of the SD card

## Inserting the SD card

The SD card to be used on the camera should always be formatted on the camera. (Formatting the SD card)

- All the recorded data will be erased and would not be able to restore when the SD card is formatted.

Card 1 access lamp

Card slot 1

Card slot cover

Card slot 2

Card 2 access lamp

Fig. 2

Fig. 1

Open the card slot cover. (Fig. 1)

Insert the SD card into the card slot. (Fig. 2)

- The card slot 1 and the card slot 2 can each insert one SD card.

- Insert straight in with the label facing left until it clicks.

Close the card slot cover.

## Removing the SD card

Open the card slot cover.

- Confirm that the card access lamp is not flashing in orange.

- Data is being written/read when the card access lamp is flashing in orange, so do not remove the SD card.

Press in the SD card further into the camera and let go.

- The SD card is released from the card slot, and pull it out straight.

Close the card slot cover.

## Cautions when using or storing

- Do not touch the terminal section at the rear of the SD card.

- Avoid high temperature and humidity.

- Avoid water droplets.

- Avoid charging with electricity.

Use or store the SD card with the card inserted into the camera and with the slot cover closed.

Top of the page