- Top
- Preparation
- Assigning function to the USER buttons

# Assigning function to the USER buttons

Selected function can be assigned to the USER buttons.

- The buttons that can be used as a USER button are as follows.

  - <USER 1> to <USER 9> buttons

    These can be used as the USER buttons when the VIEW screen is displayed.

  - Multidial (when <WB>/<USER>/<ISO/dB> switch is set to <USER>)

From the [SYSTEM SETTINGS] menu → [USER SWITCHES] → [USER1] to [USER9] or [USER TOGGLE], select the function to assign to each.

#### Functions assigned to the USER buttons in the factory setting

USER button | Function
--- | ---
<USER 1> button | [ONE PUSH AF]
<USER 2> button | [PEAK./SQUARES F.A.]
<USER 3> button | [SPOT METER]
<USER 4> button | [E.I.S.]
<USER 5> button | [WFM]
<USER 6> button | [AWB]
<USER 7> button | [SLOT SEL]
<USER 8> button | [EXPAND]
<USER 9> button | [OPEN IRIS F.A.]
Multidial | [MONITOR VOL]

Functions assigned to USER buttons
Checking the function assigned to the USER buttons
Top of the page