- Top
- Shooting
- Convenient shooting functions
- One-push auto focus function

# One-push auto focus function

The one-push auto focus function is a function to automatically adjust the focus.

The focus area is 1/3 of the screen height and 1/4 of the width.

1/4 or more of the screen width

1/3 or more of the screen height

#### Assign [ONE PUSH AF] to the USER button

Assign the one-push auto focus function so that it can be used with an arbitrary USER button.

Select the [SYSTEM SETTINGS] menu → [USER SWITCHES] → [USER1] to [USER9] → [ONE PUSH AF].

- [ONE PUSH AF] is assigned to the <USER 1> button as a factory setting.

#### Using the one-push auto focus function

Set the focus switch on the lens to AF.

Press the USER button to which [ONE PUSH AF] is assigned.

NOTE

- The one-push auto focus function operates only when a lens compatible with the auto focus is mounted.

- The one-push auto focus function will not operate in following cases.

  - When the [SYSTEM SETTINGS] menu → [COLOR SETTINGS] → [MAIN] is set to anything other than [V-Log], and EXPOSURE INDEX (gain) is set to value larger than [12800 ISO] or [20dB]

Top of the page