- Top
- Operation
- Basic operation of the menu
- Operating the menu

# Operating the menu

Various settings are possible from the menu.

There are two methods of operation, a method to operate with the multidial or grip multidial, or a method to touch the LCD monitor.

## When operating with the multidial

Operate the multidial on the camera by turning it in vertical direction or pushing it.

Fig. 1

Fig. 2

Press the <MENU> button when not recording.

The menu is displayed.

Select the menu to set.

Turn the multidial to move the cursor to the menu to set.

Press the multidial.

The lower level menu is displayed.

- The confirmation screen is displayed depending on the menu.

- Perform the similar operation if there is next level.

- In some menus, a screen to set the numeric value is displayed in the VIEW screen (Fig. 2).

- In some menus, a message is displayed if a menu cannot be executed.

- To return to one level higher, press the <EXIT> button.

Select the item to set.

Turn the multidial to move the cursor to the item to set.

Press the multidial.

A check mark is displayed at the left of the set item. (Fig. 1)

- To return to one level higher, press the <EXIT> button.

Press the <MENU> button to close the menu.

- Depending on the operating item, it will automatically return to the previous screen.

NOTE

- In a screen to set the numeric value (Fig. 2), turn the multidial in your desired direction with the multidial pushed in, and hold it to change the value with high speed.

- The grip multidial operates equally as the multidial on the camera.

## When operating by touching the LCD monitor

Operate by touching the LCD monitor.

Press the <MENU> button when not recording.

The menu is displayed.

- Menu is displayed even when the LCD monitor is touched for one second or longer and then released while the VIEW screen is displayed.

Select the menu to set.

- Touch the menu to set. The lower level menu is displayed.

- The confirmation screen is displayed depending on the menu.

- Perform the similar operation if there is next level.

- In some menus, a screen to set the numeric value is displayed in the VIEW screen.

  To change the numeric value, touch []/[] and change the setting value.

- In some menus, a message is displayed if a menu cannot be executed.

- The cursor is moved up or down by touching []/[].

- To return to one level higher, touch .

Select the item to set.

- Touch the item to set. A check mark is displayed at the left of the set item.

- To return to one level higher, touch .

Exit from the menu by touching , or pressing the <MENU> button.

- Depending on the operating item, it will automatically return to the previous screen.

Top of the page