- Top
- Overview
- Use of the camera on a system
- Basic system devices

# Basic system devices

The following are required devices for shooting.

Product name | Model No. | Remark
--- | --- | ---
VariCam 35 Camera module*1 | AU-V35C1G | “Assembling the camera module and recording module”
Recording module*1 | AU-VREC1G | “Assembling the camera module and recording module”
Shoulder mount module | AU-VSHL1G | “Mounting the shoulder mount module”
Electronic HD color view finder*2 | AU-VCVF1G | “Mounting the Electronic HD color viewfinder”
Lens (35 mm, PL mount) | ZEISS/COOKE/CANON/FUJINON, etc. | “Mounting the lens”
Stereo microphone kit | AJ-MC900G | “Using front microphone”
Battery | DIONIC HD*3 HYTRON140*3 | “Mounting and setting battery”
expressP2 memory card | AU-XP0256AG/AU-XP0256BG/AU-XP0512BG | “P2 card”
SD memory card*4 P2 memory card*4 microP2 memory card*4 | Visit the support desk at the website*4 | “P2 card” “Handling SD memory cards”

The camera module and recording module are both required in this system. The system will not run with only one of those modules.

Refer to the support desk at the following website for the latest information regarding the electric HD color view finder.

https://pro-av.panasonic.net/

A battery holder is provided as standard on the recording module.

Refer to our support desk at the following website for the latest information not included in this document.

https://pro-av.panasonic.net/

Top of the page