- Top
- Extension module
- Assembling Extension Modules
- Assembling the recording module and the recording extension module

# Assembling the recording module and the recording extension module

Fig. 1

Fig. 2

Fig. 3

Fig. 4

Align the upper lock angle at the front of the recording module with the upper lock plate at the rear of the recording extension module. (Fig. 1)

Firmly push in the recording module and connect the connection terminals of the recording extension module and recording module. (Fig. 2)

NOTE

- You cannot join the modules together if the V edge of the recording extension module is down. (Fig. 3) Push down the recording extension module release lever of the recording extension module to raise the V edge. (Fig. 4)

- Do not touch the mechanical parts near the V edge. The V edge will move quickly, which may cause injury.

## Disassembling

Fig. 1

Fig. 2

Push down the recording extension module release lever (Fig. 2) while pulling up the lock knob (red) of the recording extension module release lever. (Fig. 1)

The rear part of the recording module will slightly come up.

It will be difficult for the rear part to come up when heavy items such as batteries are mounted.

Lift the recording module.

Do not hold the control panel part. Doing so may cause the control panel to detach and fall.

Remove the upper lock angle at the front of the recording module from the upper lock plate at the rear of the recording extension module.

Top of the page