- Top
- Video Recording and Color Grading
- P2 card
- P2 card recording time

# P2 card recording time

#### P2 cards supported on the camera

The optional expressP2, P2, and microP2 memory cards can be used with the camera.

NOTE

- AJ-P2C002SG (2 GB) cards cannot be used.

- Refer to our support desk at the following website for the latest information not included in this document.

  https://pro-av.panasonic.net/

#### Main recorder

Main recording format ([MAIN CODEC]) | Setting conditions | Recording time when using a 256 GB expressP2 memory card
--- | --- | ---
[AVC-Intra4K 422] | [25.00p]/[29.97p] VFR: [OFF] | Approx. 72 min
VFR: [ON], [50fps]/[60fps] | Approx. 36 min
[AVC-Intra100] | [25.00p]/[29.97p] VFR: [OFF] | Approx. 256 min
VFR: [ON], [50fps]/[60fps] | Approx. 128 min

#### Sub recorder

Sub recording format ([SUB CODEC]) | Setting conditions | Recording time when using a 64 GB microP2 memory card
--- | --- | ---
[AVC-Intra2K 422] | [25.00p]/[29.97p] | Approx. 64 min
[AVC-Intra100] | [25.00p]/[29.97p] | Approx. 64 min
[AVC-LongG50] | [25.00p]/[29.97p] | Approx. 128 min
[AVC-LongG25] | [25.00p]/[29.97p] | Approx. 256 min

NOTE

- Indicated capacities include management and other area, so the space available for recording is less than the values in the table above.

## Dividing clips recorded on P2 cards

If a P2 card with a capacity of 8 GB or more are used with the camera, recording is automatically continued as another clip when a single continuous recording time exceeds the following time. The thumbnail operation (display, delete, restore, etc.) for a clip on the P2 devices can be performed as a operation for a single clip. Clips may be displayed as separate clips in nonlinear editing software and on a computer. When using an expressP2 card in AVC-Intra 4K 422, and if the recording is performed on a microP2 memory card that exceeds 32 GB in AVC-LongG 50 or AVC-LongG 25, the recording can be continued as a same clip by selecting [ONE FILE] from [MENU] → [REC SETTINGS] → [FILE SPLIT].

Recording format (excluding native recording) | Continuous recording time
--- | ---
AVC-Intra 4K 422 (25P/29.97P) | Approx. 1 min
AVC-Intra 100 (1080/50P, 1080/59.94P) | Approx. 3 min
AVC-Intra 100 (1080/25P, 1080/29.97P) | Approx. 5 min
AVC-LongG 50 | Approx. 10 min
AVC-LongG 25 | Approx. 20 min

Top of the page