- Top
- Viewfinder
- Adjusting and setting the viewfinder
- Adjustment method

# Adjustment method

1. Lock lever (left/right position)

2. Lock lever (front/back position)

3. Visibility adjustment ring

4. Zoom ring

#### Left/right position adjustment

Loosen the lock lever (left/right positions).

Slide the viewfinder from side to side.

Adjust to a comfortable position.

Lock the lock lever (left/right position).

#### Front/back position adjustment

Loosen the lock lever (front/rear positions).

Slide the viewfinder back and forth.

Adjust to a comfortable position.

Lock the lock lever (front/back position).

#### Visibility adjustment

Turn the visibility adjustment ring while pressing holding the upper button.

Visibility adjustment range: −3.6 D - +1.4 D

#### Zoom adjustment

Adjust by turning the zoom ring.

Adjust to a comfortable view angle while checking the video.

Perform adjustment when adjusting the focus.

Vignetting may occur around the screen of the enlarged image.

Top of the page