- Top
- Extension module
- Power supply
- Using batteries

# Using batteries

Connection of the following batteries to the device has been verified.

#### Anton/Bauer batteries

HYTRON140

DIONIC HC/DIONIC HCX/DIONIC HD

#### IDX batteries

ENDURA HL9

NOTE

- You can also use other batteries. Use of batteries that are already verified as connectable to the device is recommended.

- Before you use a battery, charge it with a battery charger. (For details on charging, refer to each operating instructions.)

- The percent (%) display will not be available for batteries with a battery level indicator function.

Top of the page