- Top
- Extension module
- Assembling Extension Modules
- Assembling the camera module and the camera extension module

# Assembling the camera module and the camera extension module

Fig. 1

Fig. 2

Fig. 3

Fig. 4

Align the upper lock angle at the front of the camera extension module with the upper lock plate at the rear of the camera module.(Fig. 1)

Firmly push in the camera extension module and connect the connection terminals of the camera module and camera extension module. (Fig. 2)

NOTE

- You cannot join the modules together if the V edge of the camera module is down. (Fig. 3) Push down the recording module release lever of the camera module to raise the V edge. (Fig. 4)

- Do not touch the mechanical parts near the V edge. The V edge will move quickly, which may cause injury.

## Disassembling

Fig. 1

Fig. 2

Push down the recording module release lever (Fig. 2) while pulling up the lock knob (red) of the recording module release lever (Fig. 1).

The rear part of the camera extension module will come up.

It will be difficult for the rear part to come up when heavy items such as batteries are mounted.

Lift the camera extension module.

Remove the upper lock angle in front of the camera extension module from the upper lock plate at the rear of the camera module.

Top of the page